{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Extent of Delivery","Tier2","Tier3"],"not_rendered":{"charts":0,"images":2,"macros":1,"external_links":0,"defined_names":6,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Extent of Delivery","index":0,"n_rows":548,"n_cols":26,"rows_kept":548,"cut":false,"hidden":false,"merged":[[353,9,353,14],[357,9,357,14],[362,9,362,14],[364,9,364,14],[371,9,371,13],[373,9,373,13],[381,9,381,11],[382,13,382,22],[382,23,382,26],[324,9,324,11],[326,9,326,11],[328,9,328,11],[337,15,337,18],[338,19,338,22],[342,9,342,27],[344,7,346,21],[347,9,347,19],[348,9,348,19],[118,17,118,21],[119,17,119,21],[120,15,120,20],[137,16,137,22],[138,16,138,22],[145,12,145,13],[145,16,145,17],[158,9,158,25],[188,13,188,14],[90,25,90,26],[91,17,91,19],[95,18,95,20],[96,18,96,20],[97,18,97,20],[98,18,98,20],[107,7,107,8],[107,9,107,13],[108,9,108,13],[60,17,60,19],[60,22,60,24],[61,17,61,19],[61,22,61,24],[62,17,62,19],[62,22,62,24],[2,3,3,18],[37,14,37,24],[27,14,27,24],[28,14,28,24],[30,14,30,24],[31,14,31,24],[32,14,32,24],[33,14,33,24],[34,14,34,24],[35,14,35,24],[36,14,36,24],[10,9,10,21],[19,14,19,24],[20,14,20,24],[21,14,21,24],[22,14,22,24],[23,14,23,24],[24,14,24,24],[25,14,25,24],[26,14,26,24],[57,1,57,4],[59,17,59,19],[517,9,517,23],[526,9,526,16],[530,9,530,16],[536,10,536,12],[536,17,536,19],[65,17,65,19],[66,17,66,19],[66,22,66,24],[69,11,69,15],[70,17,70,19],[71,17,71,19],[72,8,72,10],[72,17,72,19],[63,17,63,19],[78,14,79,19],[537,10,537,12],[537,17,537,19],[275,12,275,16],[294,17,294,18],[295,17,295,18],[382,9,382,11],[473,15,473,26],[488,9,488,23],[497,8,497,25],[498,8,498,25],[510,8,510,25],[338,15,338,18],[94,25,94,26],[109,19,109,23],[112,8,112,25],[190,11,190,25],[191,11,191,25],[197,9,197,16],[229,15,229,17],[235,16,235,18],[236,17,236,19],[249,11,249,13],[249,20,249,22],[251,11,251,13],[251,20,251,22],[257,17,257,26],[266,12,266,16],[267,12,267,16],[270,12,270,16],[271,12,271,16],[274,12,274,16],[207,11,207,25],[208,11,208,25],[215,14,215,26],[216,14,216,26],[312,13,312,26],[511,8,511,25],[388,9,388,13],[390,9,390,13],[409,9,409,11],[410,9,410,11],[410,13,410,22],[410,23,410,26]]}
[]
[]
[null,null,null,"Extent of Delivery for UE Engine"]
[]
[null,null,null," Engine type : UEC50LSH-Eco-C2-EGR"]
[]
[null,null,null,null,"  < Applicable IMO emission regulation >"]
[null,null,null,null,null,"Complied with IMO TierII regulation"]
[null,null,null,null,null,"Complied with IMO TierIII regulation"]
[]
[null,null,null,null,"◆ Engine builder ;\n"]
[]
[]
[null,null,null,null,"- Introduction -"]
[null,null,null,null,"The Extent of Delivery (EoD) of UE engine indicates the standard specification and the options "]
[null,null,null,null,"only for reference and guidance. "]
[]
[]
[null,null,null,null,"- Customer information -"]
[null,null,null,null,"Shipyard : "]
[null,null,null,null,"Owner / Company : "]
[null,null,null,null,"Others : "]
[null,null,null,null,"Contact person at shipyard : "]
[null,null,null,null,"Address : "]
[null,null,null,null,"Country : "]
[null,null,null,null,"Telephone : "]
[null,null,null,null,"Telefax : "]
[null,null,null,null,"E-mail : "]
[null,null,null,null,"Reference : "]
[]
[null,null,null,null,"Type of vessel : "]
[null,null,null,null,"Size of vessel : "]
[null,null,null,null,"Number of ships : "]
[null,null,null,null,"Total for this order : "]
[null,null,null,null,"Anticipated engine order date : "]
[null,null,null,null,"Date(s) of Engine(s) delivery : "]
[null,null,null,null,"Date(s) of ship(s) delivery : "]
[null,null,null,null,"Internal Order number/ Engine number : "]
[]
[]
[null,null,null,null,"<Remarks>"]
[null,null,null,null,"All data and information in any the below EoD is no-binding.The binding EoD for an individual project"]
[null,null,null,null,"should be offered and supplied by actual Engine builder, and the final specifications for an individual \n"]
[null,null,null,null,"project are agreed among concerned parties and determined. "]
[]
[null,null,null,"Contact：Japan Engine Corporation"]
[null,null,null,"1 Minamifutami, Futami-cho, Akashi City, Hyogo 674-0093, Japan"]
[null,null,null,"Tel : +81-78-949-0801"]
[null,null,null,"Fax : +81-78-949-0811"]
[]
[null,null,null,null,"- Engine Specification -"]
[]
[null,null,null,null,"★","Mean of check mark :"]
[null,null,null,null,null,null,"Standard item"]
[null,null,null,null,null,null,null,"or Option item"]
[]
[]
[null," < Content >"]
[null,null,null," No",null,null,null,"Particulars"]
[null,null,"01","01",null,null,null,"Number of cylinder ：",null,null,null,null,null,null,null,null,null,null,null,null," cyl."]
[null,null,"01","02",null,null,null,"P1 point rating : ",null,null,null,null,null,null,null,null,null,null,null,null," kW",null,null,null,null," min-1"]
[null,null,"01","03",null,null,null,"Max continuous rating (MCR) : ",null,null,null,null,null,null,null,null,null,null,null,null," kW",null,null,null,null," min-1"]
[null,null,"01","04",null,null,null,"Normal rating (NR) : ",null,null,null,null,null,null,null,null,null,null,null,null," kW",null,null,null,null," min-1"]
[null,null,"01","05",null,null,null,"Normal load :",null,null,null,null,null,null,null,null,null,null,null,null," % MCR"]
[]
[null,null,"01","06",null,null,null,"Contracted speed of vessel : ",null,null,null,null,null,null,null,null,null,null,null,null," knots"]
[null,null,"01","07",null,null,null,null,null,null,null,null,null,null,null,null,"at ",null,null,null," kW",null,null,null,null," min-1"]
[]
[null,null,null,null,null,null,null,"Guarantee specific fuel oil consumption on ISO condition : "]
[null,null,"01","08",null,null,null,"Planning data No. ",null,null,null,null,null,null,null,null,null,"( Correspondence mode of NOx TierII ) "]
[null,null,"01","09",null,null,null,"Contracted max continuous rating(CMCR)",null,null,null,null,null,null,null,null,null,null,null,null," g/kWh"]
[null,null,"01","10",null,null,null,"Continuous service rating(CSR) ",null,null,null,null,null,null,null,null,null,null,null,null," g/kWh"]
[null,null,"01","11",null,null,null,null,null,null,null,"% CMCR",null,null,null,null,null,null,null,null," g/kWh"]
[]
[]
[null,null,"01",{"$f":"D73+1","v":12},null,null,null,"Single engine installation (propulsion)"]
[null,null,"01",{"$f":"D76+1","v":13},null,null,null,"Twin engine installation (propulsion)"]
[]
[null,null,"01",{"$f":"D77+1","v":14},null,null,null,"Rotation clockwise",null,null,null,null,null,null,"Looking from the aft side"]
[null,null,"01",{"$f":"D79+1","v":15},null,null,null,"Rotation anti-clockwise"]
[]
[null,null,"01",{"$f":"D80+1","v":16},null,null,null,"Reversible engine(s) and fixed-pitch propeller"]
[null,null,"01",{"$f":"D82+1","v":17},null,null,null,"Non-reversible engine(s) and controllable-pitch propeller"]
[]
[]
[null,null,null,null,null,null,null,"Engine Tuning"]
[null,null,"01",20,null,null,null,"Low load optimized with EGB turbocharger"]
[]
[]
[null,null,null,null,null,null,null,"SOx Scrbber on Ship Side"]
[null,null,"01",26,null,null,null,"Not applied / Turbocharger back pressure is standard (300mmAq @ MCR)   "]
[null,null,"01",{"$f":"D91+1","v":27},null,null,null,"Equipment / Turbocharger back pressure is ",null,null,null,null,null,null,null,null,null,null,null,null,"mmAq @ MCR"]
[]
[null,null,null,null,null,null,null,"Power Take Off (PTO is not part of the engine delivery scope)"]
[null,null,"01",{"$f":"D92+1","v":28},null,null,null,"Not applied"]
[null,null,"01",{"$f":"D95+1","v":29},null,null,null,"Tunnel gear, shaft generator",null,null,null,null,null,null,null,null,null,null,null,null,null," kW"]
[null,null,"01",{"$f":"D96+1","v":30},null,null,null,"Low-speed shaft generator in shaft line",null,null,null,null,null,null,null,null,null,null,null,null,null," kW"]
[null,null,"01",31,null,null,null,"Geared generator at engine free end",null,null,null,null,null,null,null,null,null,null,null,null,null," kW"]
[null,null,"01",32,null,null,null,"Low-speed generator at engine free end",null,null,null,null,null,null,null,null,null,null,null,null,null," kW"]
[]
[null,null,null,null,null,null,null,"PTO shaft :"]
[null,null,"01",{"$f":"D99+1","v":33},null,null,null,null,null,"Supplied by Shipyard"]
[null,null,"01",{"$f":"D102+1","v":34},null,null,null,null,null,"Supplied by Engine builder"]
[]
[]
[]
[null,null,null,null,null,null,null,"Applicable Regulation / Rule and Flag"]
[null,null,"01",{"$f":"D103+1","v":35},null,null,null,"Flag : "]
[null,null,"01",{"$f":"D108+1","v":36},null,null,null,"Rule : "]
[null,null,"01",{"$f":"D109+1","v":37},null,null,null,null,null,"Notation for unattended machinary space :"]
[]
[null,null,"01",{"$f":"D110+1","v":38},null,null,null,"Applicable other  (Ice class , etc )"]
[null,null,"01",{"$f":"D112+1","v":39}]
[]
[]
[]
[null,null,null,null,null,null,null,"Engine Management & Automation"]
[null,null,null,null,null,null,null,"< Remote control system >"]
[null,null,"02","01",null,null,null,"Supplied by Engine builder",null,null,null,null,null,null,null,"Maker:",null,"Nabtesco"]
[null,null,"02","02",null,null,null,"Supplied by Shipyard",null,null,null,null,null,null,null,"Maker:"]
[null,null,"02","03",null,null,null,"Alarm & safety system maker :",null,null,null,null,null,null,null,null,null,null,null,null,null," * supplied by shipyard"]
[null,null,"02","04",null,null,null,"Alarm & safety functions for attended machinery space (AMS)"]
[null,null,"02","05",null,null,null,"Alarm & safety functions for unattended machinery space (UMS)"]
[]
[]
[null,null,null,null,null,null,null,"< Sensors on engine for remote indication and AMS* >"]
[null,null,"02","06",null,null,null,"Supplied by Engine builder "]
[null,null,"02","07",null,null,null,"Supplied by Shipyard"]
[null,null,"02","08",null,null,null,"Supplied only the thermisters by Shipyard"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"*: Alarm & Monitoriing System"]
[]
[null,null,null,null,null,null,null,"< Sensors for safety system >"]
[null,null,"02","09",null,null,null,"Supplied by Engine builder "]
[null,null,"02",10,null,null,null,"Supplied by Shipyard"]
[]
[]
[null,null,null,null,null,null,null,"< Oil mist detector >"]
[null,null,"02",11,null,null,null,"Supplied by Shipyard",null,null,null,null,null,null,"Maker :"]
[null,null,"02",12,null,null,null,"Supplied by Engine builder",null,null,null,null,null,null,"Maker :",null," [ DAIHATSU ] or  [ SPECS ]"]
[]
[]
[]
[null,null,null,null,null,null,null,"Optional Monitoring System"]
[null,null,null,null,null,null,null,"< Monitoring systems >"]
[null,null,"02",21,null,null,null,"Cylinder pressure auto-controled system. (PMI system)"]
[null,null,"02",22,null,null,null,"Sensor maker :",null,null,null,null,"KISTER",null," or ",null,"ABB"]
[]
[null,null,"02",23,null,null,null,"Bearing wear monitoring system"]
[]
[null,null,null,null,null,null,null,"Bearing lubricatig oil outlet temperature "]
[null,null,"02",24,null,null,null,"Main bearing"]
[null,null,"02",25,null,null,null,"Crankpin bearing"]
[null,null,"02",26,null,null,null,"Crosshead bearing"]
[]
[null,null,"02",27,null,null,null,"Cylinder liner wall temperature sensors"]
[]
[null,null,"02",28,null,null,null,"LC-A (Life Cycle Administrator)"]
[]
[null,null,"02",29,null,null,null,"Other /"]
[]
[]
[null,null,null,null,null,null,null,"< Potable device >"]
[null,null,"02",30,null,null,null,"Portable TF-Detector(Trace of Ferrous Detector)"]
[]
[null,null,"02",31,null,null,null,"Portable cylinder pressure measuring device"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,"Factory Acceptance Test"]
[null,null,null,null,null,null,null,"<Load test>"]
[null,null,null,null,null,null,null,"50% Load",null,null,"・・・",null,"30 min"]
[null,null,null,null,null,null,null,"75% Load",null,null,"・・・",null,"30 min"]
[null,null,null,null,null,null,null,"NR Load",null,null,"・・・",null,"30 min"]
[null,null,"03","01",null,null,null,"100% Load",null,null,"・・・",null,"60 min",null,null,null,null,null,null,null,null," ← Correspondence mode"]
[null,null,null,null,null,null,null,"110% Load",null,null,"・・・",null,"30 min (executed at preliminary test)",null,null,null,null,null,null,null,null,"      of  NOx Tier II"]
[null,null,null,null,null,null,null,"25% Load",null,null,"・・・",null,"30 min (executed at preliminary test)"]
[]
[null,null,"03","02",null,null,null,"Representative one load",null,null,null,null,null,null,null,"%","・・・","30 min",null,"← Correspondence mode of NOx TierIII"]
[]
[null,null,"03","04",null,null,null,"Additional load : "]
[]
[]
[]
[null,null,null,null,null,null,null,"<Noise measurement>"]
[null,null,"03","05",null,null,null,"Not included"]
[null,null,"03","06",null,null,null,"Measuring only for first engine"]
[null,null,"03","07",null,null,null,"Other /"]
[]
[]
[null,null,null,null,null,null,null,"< Function tests >"]
[null,null,null,null,null,null,null,"Governor test"]
[null,null,null,null,null,null,null,"Lowest revolution test (for about five minutes)"]
[null,null,"03","08",null,null,null,"Starting test (Including astern test with no load)"]
[null,null,null,null,null,null,null,"Safety device test "]
[null,null,null,null,null,null,null,"Overspeed trip test "]
[]
[null,null,"03","09",null,null,null,"Additional test : "]
[]
[]
[]
[null,null,null,null,null,null,null,"< Overhaul inspection >"]
[null,null,"03",10,null,null,null,"Overhaul items and conditions shall be in accordance with enginebuilder’s standard."]
[null,null,null,null,null,null,null,"Inspection after shop trial of components from one \ncylinder unit only"]
[]
[null,null,"03",11,null,null,null,"Additional inspection parts : "]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,"Tuning Parts for Engine Vibration"]
[null,null,null,null,null,null,null,"< Axial vibration damper >"]
[null,null,"04","01",null,null,null,"Axial vibration damper fitted as standard"]
[]
[]
[null,null,null,null,null,null,null,"< Flywheel >"]
[null,null,"04","02",null,null,null,"Standard flywheel"]
[null,null,"04","03",null,null,null,"Heavy flywheel : ",null,null,null,"inertia moment =",null,null,null,null,null,null,"kgm2 (depending on TV calculation *)"]
[null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,"Flywheel cover :"]
[null,null,"04","04",null,null,null,"Supplied by Shipyard"]
[null,null,"04","05",null,null,null,"Supplied by Engine builder "]
[]
[null,null,"04","06",null,null,null,"Apply Tuning wheel : ",null,null,null,null,"inertia moment =",null,null,null,null,null,null,"kgm2 (depending on TV calculation *)"]
[null,null,"04","07",null,null,null,"Apply Torsional vibration damper : ",null,null,null,null,null,null,null,"type =",null,null,null,null," (depending on TV calculation *)"]
[]
[]
[null,null,null,null,null,null,null,"< 2nd order moment compensator >"]
[null,null,"04","08",null,null,null,"Without 2nd order moment compensator"]
[null,null,"04","09",null,null,null,"Electric 2nd order moment compensator in steering gear room"]
[]
[]
[null,null,null,null,null,null,null,"Engine Stays"]
[null,null,"04",16,null,null,null,"Suplied by Shipyard"]
[null,null,"04",17,null,null,null,"Suplied by Engine builder"]
[]
[null,null,null,null,null,null,null,"< Friction type *>"]
[null,null,"04",18,null,null,null,null,null,null,"Exhust side : ",null,null,null,"pieces",null,"/",null,null," Pump side : ",null,null,null,"pieces"]
[null,null,null,null,null,null,null,"< Hydraulic type *>"]
[null,null,"04",19,null,null,null,null,null,null,"Exhust side : ",null,null,null,"pieces",null,"/",null,null," Pump side : ",null,null,null,"pieces"]
[null,null,null,null,null,null,"*:","refer to Engine outline drawing about stay attachment points and number"]
[]
[]
[null,null,null,null,null,null,null,"Torsional Vibration"]
[null,null,"04",26,null,null,null,"Caluclation sheet making by Engine builder"]
[null,null,"04",27,null,null,null,"*: Torsional vibration calculation sheet No."]
[]
[null,null,"04",28,null,null,null,"Caluclation sheet submit to class by Shipyard"]
[null,null,"04",29,null,null,null,"by Engine builder"]
[]
[]
[]
[]
[null,null,"04",30,null,null,null,"Measured by Shipyard"]
[null,null,"04",31,null,null,null," by Engine builder : ",null,null,null,null,"Only first ship"]
[null,null,"04",32,null,null,null," by Engine builder : "]
[]
[null,null,"04",33,null,null,null,"Make the measurement results by Shipyard "]
[null,null,"04",34,null,null,null," by Engine builder : ",null,null,null,null,"Only first ship"]
[null,null,"04",35,null,null,null," by Engine builder : "]
[]
[null,null,"04",36,null,null,null,"Submitted the measurement results to class by Shipyard"]
[null,null,"04",37,null,null,null," by Engine builder : ",null,null,null,null,"Only first ship"]
[null,null,"04",38,null,null,null," by Engine builder : "]
[]
[]
[null,null,null,null,null,null,null,"Axia Vibration Calculation"]
[null,null,"04",39,null,null,null,"Depending on class requirement"]
[]
[]
[null,null,null,null,null,null,null,"Lateral Vibration Calculation"]
[null,null,"04",41,null,null,null,"Depending on class requirement"]
[]
[]
[null,null,null,null,null,null,null,"Shaft Aligment Calculation"]
[null,null,"04",43,null,null,null,"Caluclation results made by Shipyard"]
[null,null,"04",44,null,null,null,"Caluclation results made by Engine builder"]
[]
[]
[]
[null,null,null,null,null,null,null,"Accessories and Fittings"]
[null,null,null,null,null,null,null,"< Low temperature cooling water system >"]
[null,null,"05","01",null,null,null,"Sea water cooling : sea water temperture =",null,null,null,null,null,null,null,null,null,"32",null,"ºC"]
[null,null,"05","02",null,null,null,"Central cooling : fresh water temperture =",null,null,null,null,null,null,null,null,null,null,null,"ºC"]
[]
[]
[null,null,null,null,null,null,null,"< M/E lubricating oil and hydraulic oil system >"]
[null,null,null,null,null,null,null,"Turbocharger lubricating oil system :"]
[null,null,"05","03",null,null,null,"Commmon system with main M/E lubricating oil system"]
[null,null,"05","04",null,null,null,"Separate system from M/E lubricating oil system"]
[]
[null,null,null,null,null,null,null,"Hydrulic oil system :"]
[null,null,"05","05",null,null,null,"Common system with M/E lubricating oil system "]
[null,null,"05","06",null,null,null,"Separate system from M/E lubricating oil system"]
[]
[null,null,null,null,null,null,null,"Cylinder lubricating oil system :"]
[null,null,"05","09",null,null,null,"J-ENG A-ECL system (Advance Electronically Controlled Lubricating system)"]
[]
[]
[null,null,null,null,null,null,null,"< Fuel oil  system >"]
[null,null,"05",16,null,null,null,"Specification of fuel oil : "]
[null,null,"05",17,null,null,null,"Fuel oil press. regulating valve* supplied by Engine builder"]
[null,null,null,null,null,null,null,"*This valve shall be fitted on hull side fuel return line by the Shipyard."]
[]
[null,null,null,null,null,null,null,"Heating system : "]
[null,null,"05",19,null,null,null,"Steam tracer"]
[null,null,"05",20,null,null,null,"Thermal oil"]
[null,null,"05",21,null,null,null,"Electric heating coil"]
[]
[]
[null,null,null,null,null,null,null,"< Compressed air system >"]
[null,null,"05",22,null,null,null,"Srarting air pressure [3.0MPa] "]
[null,null,"05",23,null,null,null,"Other /",null,null,null,null,"MPa"]
[null,null,"05",24,null,null,null,"Controll air pressure [0.7MPa]"]
[null,null,"05",25,null,null,null,"Other /",null,null,null,null,"MPa"]
[null,null,"05",26,null,null,null,"Service air pressure [0.7MPa]"]
[null,null,"05",27,null,null,null,"Other /",null,null,null,null,"MPa"]
[]
[]
[null,null,null,null,null,null,null,"< Scavenge air system >"]
[null,null,"05",28,null,null,null,"Fire extinguishing system with steam for scavenging air spaces [ 0.7MPa ] "]
[null,null,"05",29,null,null,null,"Fire extinguishing system with CO2 "]
[]
[]
[null,null,null,null,null,null,null,"< Turbocharger >"]
[null,null,"05",30,null,null,null,"Enginebuilder standard type : ",null,null,null,null,null,null,null,null,null,null,null,"(refer to engine planning data)"]
[null,null,"05",31,null,null,null,"Number of turbocharger(s) :"]
[]
[null,null,"05",32,null,null,null,"Gas outlet direction from the turbocharger shall be outer-side 15° from upward direction."]
[null,null,"05",33,null,null,null,"Gas outlet direction from the turbocharger shall be outer-side 30° from upward direction."]
[null,null,"05",34,null,null,null,"Other /"]
[]
[null,null,null,null,null,null,null,"The exhaust gas outlet flange, gaskets :\ntransition pipe after the turbocharger shall be installed, \nbut flexible joint and their packings, bolts, nuts are excluded."]
[null,null,"05",36]
[]
[null,null,"05",37,null,null,null,"Other / "]
[]
[]
[null,null,null,null,null,null,null,"< Scavenging air cooler >  "]
[null,null,null,null,null,null,null,"Pump and hose for cleaning device : "]
[null,null,"05",42,null,null,null,"Supplied by Engine builder"]
[null,null,"05",43,null,null,null,"Other / "]
[]
[null,null,null,null,null,null,null,"Tank for cleaning device : "]
[null,null,"05",44,null,null,null,"Supplied by Shipyard"]
[null,null,"05",45,null,null,null,"Other / "]
[]
[]
[null,null,null,null,null,null,null,"< Power supply >"]
[null,null,"05",46,null,null,null,"A/C power sorce 3φ [ 440V AC , 60Hz ] "]
[null,null,"05",47,null,null,null,"Other /"]
[null,null,"05",48,null,null,null,"A/C power sorce 1φ [ 100V AC , 60Hz ] "]
[null,null,"05",49,null,null,null,"Other /"]
[null,null,"05",50,null,null,null,"D/C power sorce [ 24V ]"]
[]
[]
[null,null,null,null,null,null,null,"< Auxiliary blower >"]
[null,null,null,null,null,null,null,"Electric motor :"]
[null,null,"05",51,null,null,null,"Totally enclosed [IP55]"]
[null,null,"05",52,null,null,null,"Other / "]
[null,null,"05",53,null,null,null,"Insulation class [F]"]
[null,null,"05",54,null,null,null,"Other / "]
[null,null,"05",55,null,null,null,"Without heater"]
[null,null,"05",56,null,null,null,"With heater"]
[]
[null,null,null,null,null,null,null,"Starter :"]
[null,null,"05",57,null,null,null,"Supplied by Shipyard"]
[null,null,"05",58,null,null,null,"Supplied by Engine builder"]
[null,null,null,null,null,null,null,null,"Starting method :"]
[null,null,"05",59,null,null,null,null,null,"Direct on line"]
[null,null,"05",60,null,null,null,null,null,"Other",null,null,"/"]
[]
[]
[null,null,null,null,null,null,null,"< Turning gear >"]
[null,null,null,null,null,null,null,"Electric motor :"]
[null,null,"05",{"$f":"D383+1","v":61},null,null,null,"Totally enclosed [IP44]"]
[null,null,"05",{"$f":"D388+1","v":62},null,null,null,"Other / "]
[null,null,"05",{"$f":"D389+1","v":63},null,null,null,"Insulation class [F]"]
[null,null,"05",{"$f":"D390+1","v":64},null,null,null,"Other / "]
[null,null,"05",{"$f":"D391+1","v":65},null,null,null,"Without heater and thermistor"]
[null,null,"05",{"$f":"D392+1","v":66},null,null,null,"With heater"]
[]
[null,null,null,null,null,null,null,"Starter : "]
[null,null,"05",{"$f":"D393+1","v":67},null,null,null,"Supplied by Engine builder",null,null,null,null,null,"(incl. manual remote control box with cable of 15 m)"]
[]
[null,null,null,null,null,null,null,"Receptor for using upper floor :\n"]
[null,null,"05",{"$f":"D396+1","v":68},null,null,null,"Not applied"]
[null,null,"05",{"$f":"D399+1","v":69},null,null,null,"Equipment"]
[]
[]
[null,null,null,null,null,null,null,"< Electric hydraulic oil pump >"]
[null,null,"05",70,null,null,null,"Electric motor : 2sets"]
[]
[null,null,null,null,null,null,null,"Starter :"]
[null,null,"05",71,null,null,null,"Starter is supplied by Shipyard"]
[null,null,"05",72,null,null,null,"Starter is supplied by Engine builder"]
[null,null,null,null,null,null,null,null,"Starting method :"]
[null,null,"05",73,null,null,null,null,null,"Direct on line"]
[null,null,"05",74,null,null,null,null,null,"Other",null,null,"/"]
[]
[]
[null,null,null,null,null,null,null,"< Components, related to LP-EGR* system >"]
[null,null,"05",75,null,null,null,"On-Engine components: supplied by Engine builder"]
[null,null,null,null,null,null,null,null,"Venturi scrubber"]
[null,null,null,null,null,null,null,null,"Demister"]
[null,null,null,null,null,null,null,null,"Scrubbing water reciever"]
[null,null,null,null,null,null,null,null,"EGR blower"]
[null,null,null,null,null,null,null,null,"EGR gas inlet/outlet valve"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"*: Low Pressure - Exhaust Gas Recirculation"]
[]
[]
[null,null,null,null,null,null,null,"< Water treatment system >"]
[null,null,"05",76,null,null,null,"[Water treatment unit], [Collecting tank unit] , [Water cooler unit] and [Control panel] "]
[null,null,null,null,null,null,null,"are supplied by Engine builder"]
[]
[]
[null,null,null,null,null,null,null,"< Other system related to LP-EGR system >"]
[null,null,"05",77,null,null,null,"[NaOH supply system], [Residue discharge system] and [Hull side piping]"]
[null,null,null,null,null,null,null,"are designed and procured by Shipyard"]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,"Engine Seating"]
[null,null,"06","01",null,null,null,"Engine prepared for mounting on epoxy chocks"]
[]
[]
[null,null,null,null,null,null,null,"Epoxy resin chocks :"]
[null,null,"06","02",null,null,null,"Supplied by Shipyard"]
[null,null,"06","03",null,null,null,"Supplied by Engine builder"]
[]
[]
[null,null,null,null,null,null,null,"Holding down bolts/nut :"]
[null,null,"06","04",null,null,null,"Supplied by Shipyard"]
[null,null,"06","05",null,null,null,"Supplied by Engine builder"]
[]
[]
[null,null,null,null,null,null,null,"Foot pieces/caps :"]
[null,null,"06","06",null,null,null,"Supplied by Shipyard"]
[null,null,"06","07",null,null,null,"Supplied by Engine builder"]
[]
[]
[null,null,null,null,null,null,null,"Jack bolt for engine aligment :"]
[null,null,"06","08",null,null,null,"Supplied by Engine builder / Number is engine builder’s standard"]
[null,null,null,null,null,null,null,null,null,null,null,null,null," refer to drawing of [arrangemrnt of holding down bolt]"]
[]
[null,null,null,null,null,null,null,"Trust stopper :"]
[null,null,"06","09",null,null,null,"Supplied by Shipyard"]
[null,null,"06",10,null,null,null,"Supplied by Engine builder"]
[]
[]
[null,null,null,null,null,null,null,"Side stopper :"]
[null,null,"06",11,null,null,null,"Supplied by Shipyard"]
[null,null,"06",12,null,null,null,"Supplied by Engine builder"]
[]
[]
[]
[null,null,null,null,null,null,null,"Lubricating Oil Outlet Position"]
[null,null,"06",13,null,null,null,"Engine bottom :",null,null,null,"Outlet position is Engine builder standard refer to drawing"]
[null,null,"06",14,null,null,null,"Engine bottom :",null,null,null,"Other position  /"]
[null,null,"06",15,null,null,null,"Engine driving end connection "]
[]
[null,null,null,null,null,null,null,"Lubricating oil outlet filter : "]
[null,null,"06",16,null,null,null,"Supplied by Shipyard"]
[null,null,"06",17,null,null,null,"Supplied by Engine builder"]
[]
[null,null,null,null,null,null,null,"Engine Coupling"]
[null,null,null,null,null,null,null,"Engine coupling bolts for thrust shaft and intermediate shaft :"]
[null,null,"06",18,null,null,null,"Supplied by Shipyard"]
[]
[]
[null,null,null,null,null,null,null,"External Conection Flanges "]
[null,null,null,null,null,null,null,"Between engine-side and ship-side :"]
[null,null,"06",19,null,null,null,"JIS"]
[null,null,"06",20,null,null,null,"Other /"]
[]
[]
[]
[null,null,null,null,null,null,null,"Spare Parts"]
[null,null,"07","01",null,null,null,"Spare parts for service required by Engine builder and recommended  \n"]
[null,null,null,null,null,null,null,"or required by the requirements of the classification society \n"]
[]
[null,null,"07","02",null,null,null,"Additional spare parts required by the owner :"]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,"Tools"]
[null,null,"07","03",null,null,null,"Standard tools for maintenance of main engine"]
[]
[null,null,"07","04",null,null,null,"Overhaul tools adapted to: normal lifting procedure, vertical lift of all components"]
[null,null,"07","05",null,null,null,"Overhaul tools adapted to: double jib crane lifting procedure"]
[null,null,"07","06",null,null,null,"Overhaul tools adapted to: reduced height lifting procedure, tilted lift of main components"]
[]
[null,null,"07","07",null,null,null,"Other special tools required by the owner :"]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,"Painting"]
[null,null,"08","01",null,null,null,"Engine builder standard finish : external surface color is [ Munsell 7.5BG7/2 ] "]
[null,null,"08","02",null,null,null,"Other / "]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,"Language"]
[null,null,null,null,null,null,null,"< Name plates for general and caution plates >"]
[null,null,"08","03",null,null,null,"English"]
[null,null,"08","04",null,null,null,"Other / "]
[]
[null,null,null,null,null,null,null,"< Maintenance manual & instruction book >"]
[null,null,"08","05",null,null,null,"English"]
[null,null,"08","06",null,null,null,"Other / "]
[]
[]
[]
[null,null,null,null,null,null,null,"Supervisors Dispatch"]
[null,null,null,null,null,null,null,"During engine installation ~ sea trial / until overhaul inspection :"]
[null,null,"09","01",null,null,null,"Standard :  ",null,null,null,null,null," days / person",null,null,null,null,null,null," number of times"]
[null,null,"09","02",null,null,null,"Other : ",null,null,null,null,null," days / person",null,null,null,null,null,null," number of times"]
[]
[]
[null,null,null,null,null,null,null,"Packing & Transport"]
[null,null,"09","03",null,null,null,"Dispatch pattern : according to consultation result by Engine builder and shipyard "]
[]
[]
[]
[null,null,10,"01",null,null,null,"Other Comment"]
[]
[null,null,10,"02"]

{"sheet":"Tier2","index":1,"n_rows":548,"n_cols":26,"rows_kept":548,"cut":false,"hidden":true,"merged":[[23,14,23,24],[24,14,24,24],[25,14,25,24],[26,14,26,24],[27,14,27,24],[28,14,28,24],[2,3,3,18],[10,9,10,21],[19,14,19,24],[20,14,20,24],[21,14,21,24],[22,14,22,24],[57,1,57,4],[59,17,59,19],[60,17,60,19],[60,22,60,24],[30,14,30,24],[31,14,31,24],[32,14,32,24],[33,14,33,24],[34,14,34,24],[35,14,35,24],[72,8,72,10],[72,17,72,19],[61,17,61,19],[61,22,61,24],[62,17,62,19],[62,22,62,24],[63,17,63,19],[65,17,65,19],[36,14,36,24],[37,14,37,24],[78,14,79,19],[94,25,94,26],[95,17,95,19],[100,25,100,26],[101,18,101,20],[102,18,102,20],[66,17,66,19],[66,22,66,24],[69,11,69,15],[70,17,70,19],[71,17,71,19],[118,8,118,25],[126,15,126,20],[103,18,103,20],[104,18,104,20],[113,7,113,8],[113,9,113,13],[114,9,114,13],[115,19,115,23],[124,17,124,21],[125,17,125,21],[338,15,338,18],[339,15,339,18],[339,19,339,22],[343,9,343,27],[345,7,347,23],[271,12,271,16],[274,12,274,16],[275,12,275,16],[294,17,294,18],[295,17,295,18],[313,13,313,26],[151,12,151,13],[151,16,151,17],[164,9,164,25],[349,9,349,19],[354,9,354,14],[358,9,358,14],[143,16,143,22],[144,16,144,22],[383,23,383,26],[383,13,383,22],[374,9,374,13],[372,9,372,13],[365,9,365,14],[363,9,363,14],[348,9,348,27],[235,16,235,18],[236,17,236,19],[257,17,257,26],[266,12,266,16],[267,12,267,16],[270,12,270,16],[205,11,205,25],[206,11,206,25],[213,14,213,26],[382,9,382,11],[418,9,418,11],[419,9,419,11],[530,9,530,16],[536,10,536,12],[536,17,536,19],[473,15,473,26],[488,9,488,23],[526,9,526,16],[517,9,517,23],[419,13,419,22],[419,23,419,26],[537,10,537,12],[537,17,537,19],[511,8,511,25],[510,8,510,25],[498,8,498,25],[497,8,497,25],[397,9,397,13],[399,9,399,13],[383,9,383,11],[189,11,189,25],[188,11,188,25],[195,9,195,16],[249,11,249,13],[249,20,249,22],[251,11,251,13],[251,20,251,22],[329,9,329,11],[327,9,327,11],[325,9,325,11],[214,14,214,26],[229,15,229,17]]}
[]
[]
[null,null,null,"Extent of Delivery for UE Engine"]
[]
[null,null,null," Engine type : UEC50LSH-Eco-C2"]
[]
[null,null,null,null,"  < Applicable IMO emission regulation >"]
[null,null,null,null,null,"Complied with IMO TierII regulation"]
[null,null,null,null,null,"Complied with IMO TierIII regulation"]
[]
[null,null,null,null,"◆ Engine builder ;\n"]
[]
[]
[null,null,null,null,"- Introduction -"]
[null,null,null,null,"The Extent of Delivery (EoD) of UE engine indicates the standard specification and the options "]
[null,null,null,null,"only for reference and guidance. "]
[]
[]
[null,null,null,null,"- Customer information -"]
[null,null,null,null,"Shipyard : "]
[null,null,null,null,"Owner / Company : "]
[null,null,null,null,"Others : "]
[null,null,null,null,"Contact person at shipyard : "]
[null,null,null,null,"Address : "]
[null,null,null,null,"Country : "]
[null,null,null,null,"Telephone : "]
[null,null,null,null,"Telefax : "]
[null,null,null,null,"E-mail : "]
[null,null,null,null,"Reference : "]
[]
[null,null,null,null,"Type of vessel : "]
[null,null,null,null,"Size of vessel : "]
[null,null,null,null,"Number of ships : "]
[null,null,null,null,"Total for this order : "]
[null,null,null,null,"Anticipated engine order date : "]
[null,null,null,null,"Date(s) of Engine(s) delivery : "]
[null,null,null,null,"Date(s) of ship(s) delivery : "]
[null,null,null,null,"Internal Order number/ Engine number : "]
[]
[]
[null,null,null,null,"<Remarks>"]
[null,null,null,null,"All data and information in any the below EoD is no-binding.The binding EoD for an individual project"]
[null,null,null,null,"should be offered and supplied by actual Engine builder, and the final specifications for an individual \n"]
[null,null,null,null,"project are agreed among concerned parties and determined. "]
[]
[null,null,null,"Contact：Japan Engine Corporation"]
[null,null,null,"1 Minamifutami, Futami-cho, Akashi City, Hyogo 674-0093, Japan"]
[null,null,null,"Tel : +81-78-949-0801"]
[null,null,null,"Fax : +81-78-949-0811"]
[]
[null,null,null,null,"- Engine Specification -"]
[]
[null,null,null,null,"★","Mean of check mark :"]
[null,null,null,null,null,null,"Standard item"]
[null,null,null,null,null,null,null,"or Option item"]
[]
[]
[null," < Content >"]
[null,null,null," No",null,null,null,"Particulars"]
[null,null,"01","01",null,null,null,"Number of cylinder ：",null,null,null,null,null,null,null,null,null,null,null,null," cyl."]
[null,null,"01","02",null,null,null,"P1 point rating : ",null,null,null,null,null,null,null,null,null,null,null,null," kW",null,null,null,null," min-1"]
[null,null,"01","03",null,null,null,"Max continuous rating (MCR) : ",null,null,null,null,null,null,null,null,null,null,null,null," kW",null,null,null,null," min-1"]
[null,null,"01","04",null,null,null,"Normal rating (NR) : ",null,null,null,null,null,null,null,null,null,null,null,null," kW",null,null,null,null," min-1"]
[null,null,"01","05",null,null,null,"Normal load :",null,null,null,null,null,null,null,null,null,null,null,null," % MCR"]
[]
[null,null,"01","06",null,null,null,"Contracted speed of vessel : ",null,null,null,null,null,null,null,null,null,null,null,null," knots"]
[null,null,"01","07",null,null,null,null,null,null,null,null,null,null,null,null,"at ",null,null,null," kW",null,null,null,null," min-1"]
[]
[null,null,null,null,null,null,null,"Guarantee specific fuel oil consumption on ISO condition : "]
[null,null,"01","08",null,null,null,"Planning data No. "]
[null,null,"01","09",null,null,null,"Contracted max continuous rating(CMCR)",null,null,null,null,null,null,null,null,null,null,null,null," g/kWh"]
[null,null,"01","10",null,null,null,"Continuous service rating(CSR) ",null,null,null,null,null,null,null,null,null,null,null,null," g/kWh"]
[null,null,"01","11",null,null,null,null,null,null,null,"% CMCR",null,null,null,null,null,null,null,null," g/kWh"]
[]
[]
[null,null,"01",{"$f":"D73+1","v":12},null,null,null,"Single engine installation (propulsion)"]
[null,null,"01",{"$f":"D76+1","v":13},null,null,null,"Twin engine installation (propulsion)"]
[]
[null,null,"01",{"$f":"D77+1","v":14},null,null,null,"Rotation clockwise",null,null,null,null,null,null,"Looking from the aft side"]
[null,null,"01",{"$f":"D79+1","v":15},null,null,null,"Rotation anti-clockwise"]
[]
[null,null,"01",{"$f":"D80+1","v":16},null,null,null,"Reversible engine(s) and fixed-pitch propeller"]
[null,null,"01",{"$f":"D82+1","v":17},null,null,null,"Non-reversible engine(s) and controllable-pitch propeller"]
[]
[]
[null,null,null,null,null,null,null,"Engine Tuning"]
[null,null,"01",{"$f":"D83+1","v":18},null,null,null,"Standard"]
[null,null,"01",{"$f":"D87+1","v":19},null,null,null,"Low load optimized"]
[null,null,"01",{"$f":"D88+1","v":20},null,null,null,"Low load optimized with EGB turbocharger"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,"SOx Scrbber on Ship Side"]
[null,null,"01",26,null,null,null,"Not applied / Turbocharger back pressure is standard (300mmAq @ MCR)   "]
[null,null,"01",{"$f":"D95+1","v":27},null,null,null,"Equipment / Turbocharger back pressure is ",null,null,null,null,null,null,null,null,null,null,null,null,"mmAq @ MCR"]
[]
[]
[]
[null,null,null,null,null,null,null,"Power Take Off (PTO is not part of the engine delivery scope)"]
[null,null,"01",{"$f":"D96+1","v":28},null,null,null,"Not applied"]
[null,null,"01",{"$f":"D101+1","v":29},null,null,null,"Tunnel gear, shaft generator",null,null,null,null,null,null,null,null,null,null,null,null,null," kW"]
[null,null,"01",{"$f":"D102+1","v":30},null,null,null,"Low-speed shaft generator in shaft line",null,null,null,null,null,null,null,null,null,null,null,null,null," kW"]
[null,null,"01",31,null,null,null,"Geared generator at engine free end",null,null,null,null,null,null,null,null,null,null,null,null,null," kW"]
[null,null,"01",32,null,null,null,"Low-speed generator at engine free end",null,null,null,null,null,null,null,null,null,null,null,null,null," kW"]
[]
[null,null,null,null,null,null,null,"PTO shaft :"]
[null,null,"01",{"$f":"D105+1","v":33},null,null,null,null,null,"Supplied by Shipyard"]
[null,null,"01",{"$f":"D108+1","v":34},null,null,null,null,null,"Supplied by Engine builder"]
[]
[]
[]
[null,null,null,null,null,null,null,"Applicable Regulation / Rule and Flag"]
[null,null,"01",{"$f":"D109+1","v":35},null,null,null,"Flag : "]
[null,null,"01",{"$f":"D114+1","v":36},null,null,null,"Rule : "]
[null,null,"01",{"$f":"D115+1","v":37},null,null,null,null,null,"Notation for unattended machinary space :"]
[]
[null,null,"01",{"$f":"D116+1","v":38},null,null,null,"Applicable other  (Ice class , etc )"]
[null,null,"01",{"$f":"D118+1","v":39}]
[]
[]
[]
[null,null,null,null,null,null,null,"Engine Management & Automation"]
[null,null,null,null,null,null,null,"< Remote control system >"]
[null,null,"02","01",null,null,null,"Supplied by Engine builder",null,null,null,null,null,null,null,"Maker:",null,"Nabtesco"]
[null,null,"02","02",null,null,null,"Supplied by Shipyard",null,null,null,null,null,null,null,"Maker:"]
[null,null,"02","03",null,null,null,"Alarm & safety system maker :",null,null,null,null,null,null,null,null,null,null,null,null,null," * supplied by shipyard"]
[null,null,"02","04",null,null,null,"Alarm & safety functions for attended machinery space (AMS)"]
[null,null,"02","05",null,null,null,"Alarm & safety functions for unattended machinery space (UMS)"]
[]
[]
[null,null,null,null,null,null,null,"< Sensors on engine for remote indication and AMS* >"]
[null,null,"02","06",null,null,null,"Supplied by Engine builder "]
[null,null,"02","07",null,null,null,"Supplied by Shipyard"]
[null,null,"02","08",null,null,null,"Supplied only the thermisters by Shipyard",null,null,null,null,null,null,null,null,null,null,null,null,null,"*: Alarm & Monitoriing System"]
[]
[null,null,null,null,null,null,null,"< Sensors for safety system >"]
[null,null,"02","09",null,null,null,"Supplied by Engine builder "]
[null,null,"02",10,null,null,null,"Supplied by Shipyard"]
[]
[]
[]
[null,null,null,null,null,null,null,"< Oil mist detector >"]
[null,null,"02",11,null,null,null,"Supplied by Shipyard",null,null,null,null,null,null,"Maker :"]
[null,null,"02",12,null,null,null,"Supplied by Engine builder",null,null,null,null,null,null,"Maker :",null," [ DAIHATSU ] or  [ SPECS ]"]
[]
[]
[]
[null,null,null,null,null,null,null,"Optional Monitoring System"]
[null,null,null,null,null,null,null,"< Monitoring systems >"]
[null,null,"02",21,null,null,null,"Cylinder pressure auto-controled system. (PMI system)"]
[null,null,"02",22,null,null,null,"Sensor maker :",null,null,null,null,"KISTER",null," or ",null,"ABB"]
[]
[null,null,"02",23,null,null,null,"Bearing wear monitoring system"]
[]
[null,null,null,null,null,null,null,"Bearing lubricatig oil outlet temperature "]
[null,null,"02",24,null,null,null,"Main bearing"]
[null,null,"02",25,null,null,null,"Crankpin bearing"]
[null,null,"02",26,null,null,null,"Crosshead bearing"]
[]
[null,null,"02",27,null,null,null,"Cylinder liner wall temperature sensors"]
[]
[null,null,"02",28,null,null,null,"LC-A (Life Cycle Administrator)"]
[]
[null,null,"02",29,null,null,null,"Other /"]
[]
[]
[null,null,null,null,null,null,null,"< Potable device >"]
[null,null,"02",30,null,null,null,"Portable TF-Detector(Trace of Ferrous Detector)"]
[]
[null,null,"02",31,null,null,null,"Portable cylinder pressure measuring device"]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,"Factory Acceptance Test"]
[null,null,null,null,null,null,null,"<Load test>"]
[null,null,null,null,null,null,null,"50% Load",null,null,"・・・",null,"30 min"]
[null,null,null,null,null,null,null,"75% Load",null,null,"・・・",null,"30 min"]
[null,null,"03","01",null,null,null,"NR Load",null,null,"・・・",null,"30 min"]
[null,null,null,null,null,null,null,"100% Load",null,null,"・・・",null,"60 min"]
[null,null,null,null,null,null,null,"110% Load",null,null,"・・・",null,"30 min (executed at preliminary test)"]
[null,null,null,null,null,null,null,"25% Load",null,null,"・・・",null,"30 min (executed at preliminary test)"]
[]
[null,null,"03","04",null,null,null,"Additional load : "]
[]
[]
[]
[null,null,null,null,null,null,null,"<Noise measurement>"]
[null,null,"03","05",null,null,null,"Not included"]
[null,null,"03","06",null,null,null,"Measuring only for first engine"]
[null,null,"03","07",null,null,null,"Other /"]
[]
[]
[null,null,null,null,null,null,null,"< Function tests >"]
[null,null,null,null,null,null,null,"Governor test"]
[null,null,null,null,null,null,null,"Lowest revolution test (for about five minutes)"]
[null,null,"03","08",null,null,null,"Starting test (Including astern test with no load)"]
[null,null,null,null,null,null,null,"Safety device test "]
[null,null,null,null,null,null,null,"Overspeed trip test "]
[]
[null,null,"03","09",null,null,null,"Additional test : "]
[]
[]
[]
[null,null,null,null,null,null,null,"< Overhaul inspection >"]
[null,null,"03",10,null,null,null,"Overhaul items and conditions shall be in accordance with enginebuilder’s standard."]
[null,null,null,null,null,null,null,"Inspection after shop trial of components from one \ncylinder unit only"]
[]
[null,null,"03",11,null,null,null,"Additional inspection parts : "]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,"Tuning Parts for Engine Vibration"]
[null,null,null,null,null,null,null,"< Axial vbration damper >"]
[null,null,"04","01",null,null,null,"Axial vibration damper fitted as standard"]
[]
[]
[null,null,null,null,null,null,null,"< Flywheel >"]
[null,null,"04","02",null,null,null,"Standard flywheel"]
[null,null,"04","03",null,null,null,"Heavy flywheel : ",null,null,null,"inertia moment =",null,null,null,null,null,null,"kgm2 (depending on TV calculation *)"]
[null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,"Flywheel cover :"]
[null,null,"04","04",null,null,null,"Supplied by Shipyard"]
[null,null,"04","05",null,null,null,"Supplied by Engine builder "]
[]
[null,null,"04","06",null,null,null,"Apply Tuning wheel : ",null,null,null,null,"inertia moment =",null,null,null,null,null,null,"kgm2 (depending on TV calculation *)"]
[null,null,"04","07",null,null,null,"Apply Torsional vibration damper : ",null,null,null,null,null,null,null,"type =",null,null,null,null," (depending on TV calculation *)"]
[]
[]
[null,null,null,null,null,null,null,"< 2nd order moment compensator >"]
[null,null,"04","08",null,null,null,"Without 2nd order moment compensator"]
[null,null,"04","09",null,null,null,"Electric 2nd order moment compensator in steering gear room"]
[]
[]
[null,null,null,null,null,null,null,"Engine Stays"]
[null,null,"04",16,null,null,null,"Suplied by Shipyard"]
[null,null,"04",17,null,null,null,"Suplied by Engine builder"]
[]
[null,null,null,null,null,null,null,"< Friction type *>"]
[null,null,"04",18,null,null,null,null,null,null,"Exhust side : ",null,null,null,"pieces",null,"/",null,null," Pump side : ",null,null,null,"pieces"]
[null,null,null,null,null,null,null,"< Hydraulic type *>"]
[null,null,"04",19,null,null,null,null,null,null,"Exhust side : ",null,null,null,"pieces",null,"/",null,null," Pump side : ",null,null,null,"pieces"]
[null,null,null,null,null,null,"*:","refer to Engine outline drawing about stay attachment points and number"]
[]
[]
[null,null,null,null,null,null,null,"Torsional Vibration"]
[null,null,"04",26,null,null,null,"Caluclation sheet making by Engine builder"]
[null,null,"04",27,null,null,null,"*: Torsional vibration calculation sheet No."]
[]
[null,null,"04",28,null,null,null,"Caluclation sheet submit to class by Shipyard"]
[null,null,"04",29,null,null,null,"by Engine builder"]
[]
[]
[]
[]
[null,null,"04",30,null,null,null,"Measured by Shipyard"]
[null,null,"04",31,null,null,null," by Engine builder : ",null,null,null,null,"Only first ship"]
[null,null,"04",32,null,null,null," by Engine builder : "]
[]
[null,null,"04",33,null,null,null,"Make the measurement results by Shipyard "]
[null,null,"04",34,null,null,null," by Engine builder : ",null,null,null,null,"Only first ship"]
[null,null,"04",35,null,null,null," by Engine builder : "]
[]
[null,null,"04",36,null,null,null,"Submitted the measurement results to class by Shipyard"]
[null,null,"04",37,null,null,null," by Engine builder : ",null,null,null,null,"Only first ship"]
[null,null,"04",38,null,null,null," by Engine builder : "]
[]
[]
[null,null,null,null,null,null,null,"Axia Vibration Calculation"]
[null,null,"04",39,null,null,null,"Depending on class requirement"]
[]
[]
[null,null,null,null,null,null,null,"Lateral Vibration Calculation"]
[null,null,"04",41,null,null,null,"Depending on class requirement"]
[]
[]
[null,null,null,null,null,null,null,"Shaft Aligment Calculation"]
[null,null,"04",43,null,null,null,"Caluclation results made by Shipyard"]
[null,null,"04",44,null,null,null,"Caluclation results made by Engine builder"]
[]
[]
[]
[null,null,null,null,null,null,null,"Accessories and Fittings"]
[null,null,null,null,null,null,null,"< Low temperature cooling water system >"]
[null,null,"05","01",null,null,null,"Sea water cooling : sea water temperture =",null,null,null,null,null,null,null,null,null,"32",null,"ºC"]
[null,null,"05","02",null,null,null,"Central cooling : fresh water temperture =",null,null,null,null,null,null,null,null,null,null,null,"ºC"]
[]
[]
[null,null,null,null,null,null,null,"< M/E lubricating oil and hydraulic oil system >"]
[null,null,null,null,null,null,null,"Turbocharger lubricating oil system :"]
[null,null,"05","03",null,null,null,"Commmon system with main M/E lubricating oil system"]
[null,null,"05","04",null,null,null,"Separate system from M/E lubricating oil system"]
[]
[null,null,null,null,null,null,null,"Hydrulic oil system :"]
[null,null,"05","05",null,null,null,"Common system with M/E lubricating oil system "]
[null,null,"05","06",null,null,null,"Separate system from M/E lubricating oil system"]
[]
[]
[null,null,null,null,null,null,null,"Cylinder lubricating oil system :"]
[null,null,"05","09",null,null,null,"J-ENG A-ECL system (Advance Electronically Controlled Lubricating system)"]
[]
[]
[null,null,null,null,null,null,null,"< Fuel oil  system >"]
[null,null,"05",16,null,null,null,"Specification of fuel oil : "]
[null,null,"05",17,null,null,null,"Fuel oil press. regulating valve* supplied by Engine builder"]
[null,null,null,null,null,null,null,"*This valve shall be fitted on hull side fuel return line by the Shipyard."]
[]
[null,null,null,null,null,null,null,"Heating system : "]
[null,null,"05",19,null,null,null,"Steam tracer"]
[null,null,"05",20,null,null,null,"Thermal oil"]
[null,null,"05",21,null,null,null,"Electric heating coil"]
[]
[]
[null,null,null,null,null,null,null,"< Compressed air system >"]
[null,null,"05",22,null,null,null,"Srarting air pressure [3.0MPa] "]
[null,null,"05",23,null,null,null,"Other /",null,null,null,null,"MPa"]
[null,null,"05",24,null,null,null,"Controll air pressure [0.7MPa]"]
[null,null,"05",25,null,null,null,"Other /",null,null,null,null,"MPa"]
[null,null,"05",26,null,null,null,"Service air pressure [0.7MPa]"]
[null,null,"05",27,null,null,null,"Other /",null,null,null,null,"MPa"]
[]
[]
[null,null,null,null,null,null,null,"< Scavenge air system >"]
[null,null,"05",28,null,null,null,"Fire extinguishing system with steam for scavenging air spaces [ 0.7MPa ] "]
[null,null,"05",29,null,null,null,"Fire extinguishing system with CO2 "]
[]
[]
[null,null,null,null,null,null,null,"< Turbocharger >"]
[null,null,"05",30,null,null,null,"Enginebuilder standard type : ",null,null,null,null,null,null,null,null,null,null,null,"(refer to engine planning data)"]
[null,null,"05",31,null,null,null,"Number of turbocharger(s) :",null,null,null,null,null,null,null,"1"]
[]
[null,null,"05",32,null,null,null,"Gas outlet direction from the turbocharger shall be outer-side 15° from upward direction."]
[null,null,"05",33,null,null,null,"Gas outlet direction from the turbocharger shall be outer-side 30° from upward direction."]
[null,null,"05",34,null,null,null,"Other /"]
[]
[null,null,null,null,null,null,null,"The exhaust gas outlet flange, gaskets :\nafter the turbocharger shall be installed, \nbut transition pipe, flexible joint and their packings, bolts, nuts are excluded."]
[null,null,"05",35]
[]
[null,null,"05",37,null,null,null,"Other / "]
[]
[]
[null,null,null,null,null,null,null,"< Scavenging air cooler >  "]
[null,null,null,null,null,null,null,"Pump and hose for cleaning device : "]
[null,null,"05",42,null,null,null,"Supplied by Engine builder"]
[null,null,"05",43,null,null,null,"Other / "]
[]
[null,null,null,null,null,null,null,"Tank for cleaning device : "]
[null,null,"05",44,null,null,null,"Supplied by Shipyard"]
[null,null,"05",45,null,null,null,"Other / "]
[]
[]
[null,null,null,null,null,null,null,"< Power supply >"]
[null,null,"05",46,null,null,null,"A/C power sorce 3φ [ 440V AC , 60Hz ] "]
[null,null,"05",47,null,null,null,"Other /"]
[null,null,"05",48,null,null,null,"A/C power sorce 1φ [ 100V AC , 60Hz ] "]
[null,null,"05",49,null,null,null,"Other /"]
[null,null,"05",50,null,null,null,"D/C power sorce [ 24V ]"]
[]
[]
[null,null,null,null,null,null,null,"< Auxiliary blower >"]
[null,null,null,null,null,null,null,"Electric motor :"]
[null,null,"05",51,null,null,null,"Totally enclosed [IP55]"]
[null,null,"05",52,null,null,null,"Other / "]
[null,null,"05",53,null,null,null,"Insulation class [F]"]
[null,null,"05",54,null,null,null,"Other / "]
[null,null,"05",55,null,null,null,"Without heater"]
[null,null,"05",56,null,null,null,"With heater"]
[]
[null,null,null,null,null,null,null,"Starter :"]
[null,null,"05",57,null,null,null,"Supplied by Shipyard"]
[null,null,"05",58,null,null,null,"Supplied by Engine builder"]
[null,null,null,null,null,null,null,null,"Starting method :"]
[null,null,"05",59,null,null,null,null,null,"Direct on line"]
[null,null,"05",60,null,null,null,null,null,"Other",null,null,"/"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,"< Turning gear >"]
[null,null,null,null,null,null,null,"Electric motor :"]
[null,null,"05",{"$f":"D384+1","v":61},null,null,null,"Totally enclosed [IP44]"]
[null,null,"05",{"$f":"D397+1","v":62},null,null,null,"Other / "]
[null,null,"05",{"$f":"D398+1","v":63},null,null,null,"Insulation class [F]"]
[null,null,"05",{"$f":"D399+1","v":64},null,null,null,"Other / "]
[null,null,"05",{"$f":"D400+1","v":65},null,null,null,"Without heater and thermistor"]
[null,null,"05",{"$f":"D401+1","v":66},null,null,null,"With heater"]
[]
[null,null,null,null,null,null,null,"Starter : "]
[null,null,"05",{"$f":"D402+1","v":67},null,null,null,"Supplied by Engine builder",null,null,null,null,null,"(incl. manual remote control box with cable of 15 m)"]
[]
[null,null,null,null,null,null,null,"Receptor for using upper floor :\n"]
[null,null,"05",{"$f":"D405+1","v":68},null,null,null,"Not applied"]
[null,null,"05",{"$f":"D408+1","v":69},null,null,null,"Equipment"]
[]
[]
[null,null,null,null,null,null,null,"< Electric hydraulic oil pump >"]
[null,null,"05",70,null,null,null,"Electric motor : 2sets"]
[]
[null,null,null,null,null,null,null,"Starter :"]
[null,null,"05",71,null,null,null,"Starter is supplied by Shipyard"]
[null,null,"05",72,null,null,null,"Starter is supplied by Engine builder"]
[null,null,null,null,null,null,null,null,"Starting method :"]
[null,null,"05",73,null,null,null,null,null,"Direct on line"]
[null,null,"05",74,null,null,null,null,null,"Other",null,null,"/"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,"Engine Seating"]
[null,null,"06","01",null,null,null,"Engine prepared for mounting on epoxy chocks"]
[]
[]
[null,null,null,null,null,null,null,"Epoxy resin chocks :"]
[null,null,"06","02",null,null,null,"Supplied by Shipyard"]
[null,null,"06","03",null,null,null,"Supplied by Engine builder"]
[]
[]
[null,null,null,null,null,null,null,"Holding down bolts/nut :"]
[null,null,"06","04",null,null,null,"Supplied by Shipyard"]
[null,null,"06","05",null,null,null,"Supplied by Engine builder"]
[]
[]
[null,null,null,null,null,null,null,"Foot pieces/caps :"]
[null,null,"06","06",null,null,null,"Supplied by Shipyard"]
[null,null,"06","07",null,null,null,"Supplied by Engine builder"]
[]
[]
[null,null,null,null,null,null,null,"Jack bolt for engine aligment :"]
[null,null,"06","08",null,null,null,"Supplied by Engine builder / Number is engine builder’s standard"]
[null,null,null,null,null,null,null,null,null,null,null,null,null," refer to drawing of [arrangemrnt of holding down bolt]"]
[]
[null,null,null,null,null,null,null,"Trust stopper :"]
[null,null,"06","09",null,null,null,"Supplied by Shipyard"]
[null,null,"06",10,null,null,null,"Supplied by Engine builder"]
[]
[]
[null,null,null,null,null,null,null,"Side stopper :"]
[null,null,"06",11,null,null,null,"Supplied by Shipyard"]
[null,null,"06",12,null,null,null,"Supplied by Engine builder"]
[]
[]
[]
[null,null,null,null,null,null,null,"Lubricating Oil Outlet Position"]
[null,null,"06",13,null,null,null,"Engine bottom :",null,null,null,"Outlet position is Engine builder standard refer to drawing"]
[null,null,"06",14,null,null,null,"Engine bottom :",null,null,null,"Other position  /"]
[null,null,"06",15,null,null,null,"Engine driving end connection "]
[]
[null,null,null,null,null,null,null,"Lubricating oil outlet filter : "]
[null,null,"06",16,null,null,null,"Supplied by Shipyard"]
[null,null,"06",17,null,null,null,"Supplied by Engine builder"]
[]
[null,null,null,null,null,null,null,"Engine Coupling"]
[null,null,null,null,null,null,null,"Engine coupling bolts for thrust shaft and intermediate shaft :"]
[null,null,"06",18,null,null,null,"Supplied by Shipyard"]
[]
[]
[null,null,null,null,null,null,null,"External Conection Flanges "]
[null,null,null,null,null,null,null,"Between engine-side and ship-side :"]
[null,null,"06",19,null,null,null,"JIS"]
[null,null,"06",20,null,null,null,"Other /"]
[]
[]
[]
[null,null,null,null,null,null,null,"Spare Parts"]
[null,null,"07","01",null,null,null,"Spare parts for service required by Engine builder and recommended  \n"]
[null,null,null,null,null,null,null,"or required by the requirements of the classification society \n"]
[]
[null,null,"07","02",null,null,null,"Additional spare parts required by the owner :"]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,"Tools"]
[null,null,"07","03",null,null,null,"Standard tools for maintenance of main engine"]
[]
[null,null,"07","04",null,null,null,"Overhaul tools adapted to: normal lifting procedure, vertical lift of all components"]
[null,null,"07","05",null,null,null,"Overhaul tools adapted to: double jib crane lifting procedure"]
[null,null,"07","06",null,null,null,"Overhaul tools adapted to: reduced height lifting procedure, tilted lift of main components"]
[]
[null,null,"07","07",null,null,null,"Other special tools required by the owner :"]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,"Painting"]
[null,null,"08","01",null,null,null,"Engine builder standard finish : external surface color is [ Munsell 7.5BG7/2 ] "]
[null,null,"08","02",null,null,null,"Other / "]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,"Language"]
[null,null,null,null,null,null,null,"< Name plates for general and caution plates >"]
[null,null,"08","03",null,null,null,"English"]
[null,null,"08","04",null,null,null,"Other / "]
[]
[null,null,null,null,null,null,null,"< Maintenance manual & instruction book >"]
[null,null,"08","05",null,null,null,"English"]
[null,null,"08","06",null,null,null,"Other / "]
[]
[]
[]
[null,null,null,null,null,null,null,"Supervisors Dispatch"]
[null,null,null,null,null,null,null,"During engine installation ~ sea trial / until overhaul inspection :"]
[null,null,"09","01",null,null,null,"Standard :  ",null,null,null,null,null," days / person",null,null,null,null,null,null," number of times"]
[null,null,"09","02",null,null,null,"Other : ",null,null,null,null,null," days / person",null,null,null,null,null,null," number of times"]
[]
[]
[null,null,null,null,null,null,null,"Packing & Transport"]
[null,null,"09","03",null,null,null,"Dispatch pattern : according to consultation result by Engine builder and shipyard "]
[]
[]
[]
[null,null,10,"01",null,null,null,"Other Comment"]
[]
[null,null,10,"02"]

{"sheet":"Tier3","index":2,"n_rows":548,"n_cols":26,"rows_kept":548,"cut":false,"hidden":true,"merged":[[23,14,23,24],[24,14,24,24],[25,14,25,24],[26,14,26,24],[27,14,27,24],[28,14,28,24],[2,3,3,18],[10,9,10,21],[19,14,19,24],[20,14,20,24],[21,14,21,24],[22,14,22,24],[57,1,57,4],[59,17,59,19],[60,17,60,19],[60,22,60,24],[30,14,30,24],[31,14,31,24],[32,14,32,24],[33,14,33,24],[34,14,34,24],[35,14,35,24],[72,8,72,10],[72,17,72,19],[61,17,61,19],[61,22,61,24],[62,17,62,19],[62,22,62,24],[63,17,63,19],[65,17,65,19],[36,14,36,24],[37,14,37,24],[78,14,79,19],[90,25,90,26],[91,17,91,19],[94,25,94,26],[95,18,95,20],[96,18,96,20],[66,17,66,19],[66,22,66,24],[69,11,69,15],[70,17,70,19],[71,17,71,19],[112,8,112,25],[188,13,188,14],[190,11,190,25],[191,11,191,25],[97,18,97,20],[98,18,98,20],[107,9,107,13],[108,9,108,13],[109,19,109,23],[137,16,137,22],[120,15,120,20],[138,16,138,22],[145,12,145,13],[145,16,145,17],[158,9,158,25],[107,7,107,8],[118,17,118,21],[119,17,119,21],[197,9,197,16],[207,11,207,25],[208,11,208,25],[215,14,215,26],[216,14,216,26],[229,15,229,17],[271,12,271,16],[274,12,274,16],[275,12,275,16],[249,11,249,13],[249,20,249,22],[251,11,251,13],[251,20,251,22],[257,17,257,26],[266,12,266,16],[267,12,267,16],[270,12,270,16],[235,16,235,18],[236,17,236,19],[294,17,294,18],[295,17,295,18],[312,13,312,26],[324,9,324,11],[326,9,326,11],[328,9,328,11],[382,9,382,11],[382,13,382,22],[382,23,382,26],[348,9,348,19],[353,9,353,14],[357,9,357,14],[362,9,362,14],[364,9,364,14],[371,9,371,13],[373,9,373,13],[381,9,381,11],[337,15,337,18],[338,15,338,18],[338,19,338,22],[342,9,342,27],[344,7,346,21],[347,9,347,19],[388,9,388,13],[390,9,390,13],[409,9,409,11],[410,9,410,11],[410,13,410,22],[410,23,410,26],[536,10,536,12],[536,17,536,19],[537,10,537,12],[537,17,537,19],[473,15,473,26],[488,9,488,23],[497,8,497,25],[498,8,498,25],[510,8,510,25],[511,8,511,25],[517,9,517,23],[526,9,526,16],[530,9,530,16]]}
[]
[]
[null,null,null,"Extent of Delivery for UE Engine"]
[]
[null,null,null," Engine type : UEC50LSH-Eco-C2-EGR"]
[]
[null,null,null,null,"  < Applicable IMO emission regulation >"]
[null,null,null,null,null,"Complied with IMO TierII regulation"]
[null,null,null,null,null,"Complied with IMO TierIII regulation"]
[]
[null,null,null,null,"◆ Engine builder ;\n"]
[]
[]
[null,null,null,null,"- Introduction -"]
[null,null,null,null,"The Extent of Delivery (EoD) of UE engine indicates the standard specification and the options "]
[null,null,null,null,"only for reference and guidance. "]
[]
[]
[null,null,null,null,"- Customer information -"]
[null,null,null,null,"Shipyard : "]
[null,null,null,null,"Owner / Company : "]
[null,null,null,null,"Others : "]
[null,null,null,null,"Contact person at shipyard : "]
[null,null,null,null,"Address : "]
[null,null,null,null,"Country : "]
[null,null,null,null,"Telephone : "]
[null,null,null,null,"Telefax : "]
[null,null,null,null,"E-mail : "]
[null,null,null,null,"Reference : "]
[]
[null,null,null,null,"Type of vessel : "]
[null,null,null,null,"Size of vessel : "]
[null,null,null,null,"Number of ships : "]
[null,null,null,null,"Total for this order : "]
[null,null,null,null,"Anticipated engine order date : "]
[null,null,null,null,"Date(s) of Engine(s) delivery : "]
[null,null,null,null,"Date(s) of ship(s) delivery : "]
[null,null,null,null,"Internal Order number/ Engine number : "]
[]
[]
[null,null,null,null,"<Remarks>"]
[null,null,null,null,"All data and information in any the below EoD is no-binding.The binding EoD for an individual project"]
[null,null,null,null,"should be offered and supplied by actual Engine builder, and the final specifications for an individual \n"]
[null,null,null,null,"project are agreed among concerned parties and determined. "]
[]
[null,null,null,"Contact：Japan Engine Corporation"]
[null,null,null,"1 Minamifutami, Futami-cho, Akashi City, Hyogo 674-0093, Japan"]
[null,null,null,"Tel : +81-78-949-0801"]
[null,null,null,"Fax : +81-78-949-0811"]
[]
[null,null,null,null,"- Engine Specification -"]
[]
[null,null,null,null,"★","Mean of check mark :"]
[null,null,null,null,null,null,"Standard item"]
[null,null,null,null,null,null,null,"or Option item"]
[]
[]
[null," < Content >"]
[null,null,null," No",null,null,null,"Particulars"]
[null,null,"01","01",null,null,null,"Number of cylinder ：",null,null,null,null,null,null,null,null,null,null,null,null," cyl."]
[null,null,"01","02",null,null,null,"P1 point rating : ",null,null,null,null,null,null,null,null,null,null,null,null," kW",null,null,null,null," min-1"]
[null,null,"01","03",null,null,null,"Max continuous rating (MCR) : ",null,null,null,null,null,null,null,null,null,null,null,null," kW",null,null,null,null," min-1"]
[null,null,"01","04",null,null,null,"Normal rating (NR) : ",null,null,null,null,null,null,null,null,null,null,null,null," kW",null,null,null,null," min-1"]
[null,null,"01","05",null,null,null,"Normal load :",null,null,null,null,null,null,null,null,null,null,null,null," % MCR"]
[]
[null,null,"01","06",null,null,null,"Contracted speed of vessel : ",null,null,null,null,null,null,null,null,null,null,null,null," knots"]
[null,null,"01","07",null,null,null,null,null,null,null,null,null,null,null,null,"at ",null,null,null," kW",null,null,null,null," min-1"]
[]
[null,null,null,null,null,null,null,"Guarantee specific fuel oil consumption on ISO condition : "]
[null,null,"01","08",null,null,null,"Planning data No. ",null,null,null,null,null,null,null,null,null,"( Correspondence mode of NOx TierII ) "]
[null,null,"01","09",null,null,null,"Contracted max continuous rating(CMCR)",null,null,null,null,null,null,null,null,null,null,null,null," g/kWh"]
[null,null,"01","10",null,null,null,"Continuous service rating(CSR) ",null,null,null,null,null,null,null,null,null,null,null,null," g/kWh"]
[null,null,"01","11",null,null,null,null,null,null,null,"% CMCR",null,null,null,null,null,null,null,null," g/kWh"]
[]
[]
[null,null,"01",{"$f":"D73+1","v":12},null,null,null,"Single engine installation (propulsion)"]
[null,null,"01",{"$f":"D76+1","v":13},null,null,null,"Twin engine installation (propulsion)"]
[]
[null,null,"01",{"$f":"D77+1","v":14},null,null,null,"Rotation clockwise",null,null,null,null,null,null,"Looking from the aft side"]
[null,null,"01",{"$f":"D79+1","v":15},null,null,null,"Rotation anti-clockwise"]
[]
[null,null,"01",{"$f":"D80+1","v":16},null,null,null,"Reversible engine(s) and fixed-pitch propeller"]
[null,null,"01",{"$f":"D82+1","v":17},null,null,null,"Non-reversible engine(s) and controllable-pitch propeller"]
[]
[]
[null,null,null,null,null,null,null,"Engine Tuning"]
[null,null,"01",20,null,null,null,"Low load optimized with EGB turbocharger"]
[]
[]
[null,null,null,null,null,null,null,"SOx Scrbber on Ship Side"]
[null,null,"01",26,null,null,null,"Not applied / Turbocharger back pressure is standard (300mmAq @ MCR)   "]
[null,null,"01",{"$f":"D91+1","v":27},null,null,null,"Equipment / Turbocharger back pressure is ",null,null,null,null,null,null,null,null,null,null,null,null,"mmAq @ MCR"]
[]
[null,null,null,null,null,null,null,"Power Take Off (PTO is not part of the engine delivery scope)"]
[null,null,"01",{"$f":"D92+1","v":28},null,null,null,"Not applied"]
[null,null,"01",{"$f":"D95+1","v":29},null,null,null,"Tunnel gear, shaft generator",null,null,null,null,null,null,null,null,null,null,null,null,null," kW"]
[null,null,"01",{"$f":"D96+1","v":30},null,null,null,"Low-speed shaft generator in shaft line",null,null,null,null,null,null,null,null,null,null,null,null,null," kW"]
[null,null,"01",31,null,null,null,"Geared generator at engine free end",null,null,null,null,null,null,null,null,null,null,null,null,null," kW"]
[null,null,"01",32,null,null,null,"Low-speed generator at engine free end",null,null,null,null,null,null,null,null,null,null,null,null,null," kW"]
[]
[null,null,null,null,null,null,null,"PTO shaft :"]
[null,null,"01",{"$f":"D99+1","v":33},null,null,null,null,null,"Supplied by Shipyard"]
[null,null,"01",{"$f":"D102+1","v":34},null,null,null,null,null,"Supplied by Engine builder"]
[]
[]
[]
[null,null,null,null,null,null,null,"Applicable Regulation / Rule and Flag"]
[null,null,"01",{"$f":"D103+1","v":35},null,null,null,"Flag : "]
[null,null,"01",{"$f":"D108+1","v":36},null,null,null,"Rule : "]
[null,null,"01",{"$f":"D109+1","v":37},null,null,null,null,null,"Notation for unattended machinary space :"]
[]
[null,null,"01",{"$f":"D110+1","v":38},null,null,null,"Applicable other  (Ice class , etc )"]
[null,null,"01",{"$f":"D112+1","v":39}]
[]
[]
[]
[null,null,null,null,null,null,null,"Engine Management & Automation"]
[null,null,null,null,null,null,null,"< Remote control system >"]
[null,null,"02","01",null,null,null,"Supplied by Engine builder",null,null,null,null,null,null,null,"Maker:",null,"Nabtesco"]
[null,null,"02","02",null,null,null,"Supplied by Shipyard",null,null,null,null,null,null,null,"Maker:"]
[null,null,"02","03",null,null,null,"Alarm & safety system maker :",null,null,null,null,null,null,null,null,null,null,null,null,null," * supplied by shipyard"]
[null,null,"02","04",null,null,null,"Alarm & safety functions for attended machinery space (AMS)"]
[null,null,"02","05",null,null,null,"Alarm & safety functions for unattended machinery space (UMS)"]
[]
[]
[null,null,null,null,null,null,null,"< Sensors on engine for remote indication and AMS* >"]
[null,null,"02","06",null,null,null,"Supplied by Engine builder "]
[null,null,"02","07",null,null,null,"Supplied by Shipyard"]
[null,null,"02","08",null,null,null,"Supplied only the thermisters by Shipyard"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"*: Alarm & Monitoriing System"]
[]
[null,null,null,null,null,null,null,"< Sensors for safety system >"]
[null,null,"02","09",null,null,null,"Supplied by Engine builder "]
[null,null,"02",10,null,null,null,"Supplied by Shipyard"]
[]
[]
[null,null,null,null,null,null,null,"< Oil mist detector >"]
[null,null,"02",11,null,null,null,"Supplied by Shipyard",null,null,null,null,null,null,"Maker :"]
[null,null,"02",12,null,null,null,"Supplied by Engine builder",null,null,null,null,null,null,"Maker :",null," [ DAIHATSU ] or  [ SPECS ]"]
[]
[]
[]
[null,null,null,null,null,null,null,"Optional Monitoring System"]
[null,null,null,null,null,null,null,"< Monitoring systems >"]
[null,null,"02",21,null,null,null,"Cylinder pressure auto-controled system. (PMI system)"]
[null,null,"02",22,null,null,null,"Sensor maker :",null,null,null,null,"KISTER",null," or ",null,"ABB"]
[]
[null,null,"02",23,null,null,null,"Bearing wear monitoring system"]
[]
[null,null,null,null,null,null,null,"Bearing lubricatig oil outlet temperature "]
[null,null,"02",24,null,null,null,"Main bearing"]
[null,null,"02",25,null,null,null,"Crankpin bearing"]
[null,null,"02",26,null,null,null,"Crosshead bearing"]
[]
[null,null,"02",27,null,null,null,"Cylinder liner wall temperature sensors"]
[]
[null,null,"02",28,null,null,null,"LC-A (Life Cycle Administrator)"]
[]
[null,null,"02",29,null,null,null,"Other /"]
[]
[]
[null,null,null,null,null,null,null,"< Potable device >"]
[null,null,"02",30,null,null,null,"Portable TF-Detector(Trace of Ferrous Detector)"]
[]
[null,null,"02",31,null,null,null,"Portable cylinder pressure measuring device"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,"Factory Acceptance Test"]
[null,null,null,null,null,null,null,"<Load test>"]
[null,null,null,null,null,null,null,"50% Load",null,null,"・・・",null,"30 min"]
[null,null,null,null,null,null,null,"75% Load",null,null,"・・・",null,"30 min"]
[null,null,null,null,null,null,null,"NR Load",null,null,"・・・",null,"30 min"]
[null,null,"03","01",null,null,null,"100% Load",null,null,"・・・",null,"60 min",null,null,null,null,null,null,null,null," ← Correspondence mode"]
[null,null,null,null,null,null,null,"110% Load",null,null,"・・・",null,"30 min (executed at preliminary test)",null,null,null,null,null,null,null,null,"      of  NOx Tier II"]
[null,null,null,null,null,null,null,"25% Load",null,null,"・・・",null,"30 min (executed at preliminary test)"]
[]
[null,null,"03","02",null,null,null,"Representative one load",null,null,null,null,null,null,null,"%","・・・","30 min",null,"← Correspondence mode of NOx TierIII"]
[]
[null,null,"03","04",null,null,null,"Additional load : "]
[]
[]
[]
[null,null,null,null,null,null,null,"<Noise measurement>"]
[null,null,"03","05",null,null,null,"Not included"]
[null,null,"03","06",null,null,null,"Measuring only for first engine"]
[null,null,"03","07",null,null,null,"Other /"]
[]
[]
[null,null,null,null,null,null,null,"< Function tests >"]
[null,null,null,null,null,null,null,"Governor test"]
[null,null,null,null,null,null,null,"Lowest revolution test (for about five minutes)"]
[null,null,"03","08",null,null,null,"Starting test (Including astern test with no load)"]
[null,null,null,null,null,null,null,"Safety device test "]
[null,null,null,null,null,null,null,"Overspeed trip test "]
[]
[null,null,"03","09",null,null,null,"Additional test : "]
[]
[]
[]
[null,null,null,null,null,null,null,"< Overhaul inspection >"]
[null,null,"03",10,null,null,null,"Overhaul items and conditions shall be in accordance with enginebuilder’s standard."]
[null,null,null,null,null,null,null,"Inspection after shop trial of components from one \ncylinder unit only"]
[]
[null,null,"03",11,null,null,null,"Additional inspection parts : "]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,"Tuning Parts for Engine Vibration"]
[null,null,null,null,null,null,null,"< Axial vibration damper >"]
[null,null,"04","01",null,null,null,"Axial vibration damper fitted as standard"]
[]
[]
[null,null,null,null,null,null,null,"< Flywheel >"]
[null,null,"04","02",null,null,null,"Standard flywheel"]
[null,null,"04","03",null,null,null,"Heavy flywheel : ",null,null,null,"inertia moment =",null,null,null,null,null,null,"kgm2 (depending on TV calculation *)"]
[null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,"Flywheel cover :"]
[null,null,"04","04",null,null,null,"Supplied by Shipyard"]
[null,null,"04","05",null,null,null,"Supplied by Engine builder "]
[]
[null,null,"04","06",null,null,null,"Apply Tuning wheel : ",null,null,null,null,"inertia moment =",null,null,null,null,null,null,"kgm2 (depending on TV calculation *)"]
[null,null,"04","07",null,null,null,"Apply Torsional vibration damper : ",null,null,null,null,null,null,null,"type =",null,null,null,null," (depending on TV calculation *)"]
[]
[]
[null,null,null,null,null,null,null,"< 2nd order moment compensator >"]
[null,null,"04","08",null,null,null,"Without 2nd order moment compensator"]
[null,null,"04","09",null,null,null,"Electric 2nd order moment compensator in steering gear room"]
[]
[]
[null,null,null,null,null,null,null,"Engine Stays"]
[null,null,"04",16,null,null,null,"Suplied by Shipyard"]
[null,null,"04",17,null,null,null,"Suplied by Engine builder"]
[]
[null,null,null,null,null,null,null,"< Friction type *>"]
[null,null,"04",18,null,null,null,null,null,null,"Exhust side : ",null,null,null,"pieces",null,"/",null,null," Pump side : ",null,null,null,"pieces"]
[null,null,null,null,null,null,null,"< Hydraulic type *>"]
[null,null,"04",19,null,null,null,null,null,null,"Exhust side : ",null,null,null,"pieces",null,"/",null,null," Pump side : ",null,null,null,"pieces"]
[null,null,null,null,null,null,"*:","refer to Engine outline drawing about stay attachment points and number"]
[]
[]
[null,null,null,null,null,null,null,"Torsional Vibration"]
[null,null,"04",26,null,null,null,"Caluclation sheet making by Engine builder"]
[null,null,"04",27,null,null,null,"*: Torsional vibration calculation sheet No."]
[]
[null,null,"04",28,null,null,null,"Caluclation sheet submit to class by Shipyard"]
[null,null,"04",29,null,null,null,"by Engine builder"]
[]
[]
[]
[]
[null,null,"04",30,null,null,null,"Measured by Shipyard"]
[null,null,"04",31,null,null,null," by Engine builder : ",null,null,null,null,"Only first ship"]
[null,null,"04",32,null,null,null," by Engine builder : "]
[]
[null,null,"04",33,null,null,null,"Make the measurement results by Shipyard "]
[null,null,"04",34,null,null,null," by Engine builder : ",null,null,null,null,"Only first ship"]
[null,null,"04",35,null,null,null," by Engine builder : "]
[]
[null,null,"04",36,null,null,null,"Submitted the measurement results to class by Shipyard"]
[null,null,"04",37,null,null,null," by Engine builder : ",null,null,null,null,"Only first ship"]
[null,null,"04",38,null,null,null," by Engine builder : "]
[]
[]
[null,null,null,null,null,null,null,"Axia Vibration Calculation"]
[null,null,"04",39,null,null,null,"Depending on class requirement"]
[]
[]
[null,null,null,null,null,null,null,"Lateral Vibration Calculation"]
[null,null,"04",41,null,null,null,"Depending on class requirement"]
[]
[]
[null,null,null,null,null,null,null,"Shaft Aligment Calculation"]
[null,null,"04",43,null,null,null,"Caluclation results made by Shipyard"]
[null,null,"04",44,null,null,null,"Caluclation results made by Engine builder"]
[]
[]
[]
[null,null,null,null,null,null,null,"Accessories and Fittings"]
[null,null,null,null,null,null,null,"< Low temperature cooling water system >"]
[null,null,"05","01",null,null,null,"Sea water cooling : sea water temperture =",null,null,null,null,null,null,null,null,null,"32",null,"ºC"]
[null,null,"05","02",null,null,null,"Central cooling : fresh water temperture =",null,null,null,null,null,null,null,null,null,null,null,"ºC"]
[]
[]
[null,null,null,null,null,null,null,"< M/E lubricating oil and hydraulic oil system >"]
[null,null,null,null,null,null,null,"Turbocharger lubricating oil system :"]
[null,null,"05","03",null,null,null,"Commmon system with main M/E lubricating oil system"]
[null,null,"05","04",null,null,null,"Separate system from M/E lubricating oil system"]
[]
[null,null,null,null,null,null,null,"Hydrulic oil system :"]
[null,null,"05","05",null,null,null,"Common system with M/E lubricating oil system "]
[null,null,"05","06",null,null,null,"Separate system from M/E lubricating oil system"]
[]
[null,null,null,null,null,null,null,"Cylinder lubricating oil system :"]
[null,null,"05","09",null,null,null,"J-ENG A-ECL system (Advance Electronically Controlled Lubricating system)"]
[]
[]
[null,null,null,null,null,null,null,"< Fuel oil  system >"]
[null,null,"05",16,null,null,null,"Specification of fuel oil : "]
[null,null,"05",17,null,null,null,"Fuel oil press. regulating valve* supplied by Engine builder"]
[null,null,null,null,null,null,null,"*This valve shall be fitted on hull side fuel return line by the Shipyard."]
[]
[null,null,null,null,null,null,null,"Heating system : "]
[null,null,"05",19,null,null,null,"Steam tracer"]
[null,null,"05",20,null,null,null,"Thermal oil"]
[null,null,"05",21,null,null,null,"Electric heating coil"]
[]
[]
[null,null,null,null,null,null,null,"< Compressed air system >"]
[null,null,"05",22,null,null,null,"Srarting air pressure [3.0MPa] "]
[null,null,"05",23,null,null,null,"Other /",null,null,null,null,"MPa"]
[null,null,"05",24,null,null,null,"Controll air pressure [0.7MPa]"]
[null,null,"05",25,null,null,null,"Other /",null,null,null,null,"MPa"]
[null,null,"05",26,null,null,null,"Service air pressure [0.7MPa]"]
[null,null,"05",27,null,null,null,"Other /",null,null,null,null,"MPa"]
[]
[]
[null,null,null,null,null,null,null,"< Scavenge air system >"]
[null,null,"05",28,null,null,null,"Fire extinguishing system with steam for scavenging air spaces [ 0.7MPa ] "]
[null,null,"05",29,null,null,null,"Fire extinguishing system with CO2 "]
[]
[]
[null,null,null,null,null,null,null,"< Turbocharger >"]
[null,null,"05",30,null,null,null,"Enginebuilder standard type : ",null,null,null,null,null,null,null,null,null,null,null,"(refer to engine planning data)"]
[null,null,"05",31,null,null,null,"Number of turbocharger(s) :"]
[]
[null,null,"05",32,null,null,null,"Gas outlet direction from the turbocharger shall be outer-side 15° from upward direction."]
[null,null,"05",33,null,null,null,"Gas outlet direction from the turbocharger shall be outer-side 30° from upward direction."]
[null,null,"05",34,null,null,null,"Other /"]
[]
[null,null,null,null,null,null,null,"The exhaust gas outlet flange, gaskets :\ntransition pipe after the turbocharger shall be installed, \nbut flexible joint and their packings, bolts, nuts are excluded."]
[null,null,"05",36]
[]
[null,null,"05",37,null,null,null,"Other / "]
[]
[]
[null,null,null,null,null,null,null,"< Scavenging air cooler >  "]
[null,null,null,null,null,null,null,"Pump and hose for cleaning device : "]
[null,null,"05",42,null,null,null,"Supplied by Engine builder"]
[null,null,"05",43,null,null,null,"Other / "]
[]
[null,null,null,null,null,null,null,"Tank for cleaning device : "]
[null,null,"05",44,null,null,null,"Supplied by Shipyard"]
[null,null,"05",45,null,null,null,"Other / "]
[]
[]
[null,null,null,null,null,null,null,"< Power supply >"]
[null,null,"05",46,null,null,null,"A/C power sorce 3φ [ 440V AC , 60Hz ] "]
[null,null,"05",47,null,null,null,"Other /"]
[null,null,"05",48,null,null,null,"A/C power sorce 1φ [ 100V AC , 60Hz ] "]
[null,null,"05",49,null,null,null,"Other /"]
[null,null,"05",50,null,null,null,"D/C power sorce [ 24V ]"]
[]
[]
[null,null,null,null,null,null,null,"< Auxiliary blower >"]
[null,null,null,null,null,null,null,"Electric motor :"]
[null,null,"05",51,null,null,null,"Totally enclosed [IP55]"]
[null,null,"05",52,null,null,null,"Other / "]
[null,null,"05",53,null,null,null,"Insulation class [F]"]
[null,null,"05",54,null,null,null,"Other / "]
[null,null,"05",55,null,null,null,"Without heater"]
[null,null,"05",56,null,null,null,"With heater"]
[]
[null,null,null,null,null,null,null,"Starter :"]
[null,null,"05",57,null,null,null,"Supplied by Shipyard"]
[null,null,"05",58,null,null,null,"Supplied by Engine builder"]
[null,null,null,null,null,null,null,null,"Starting method :"]
[null,null,"05",59,null,null,null,null,null,"Direct on line"]
[null,null,"05",60,null,null,null,null,null,"Other",null,null,"/"]
[]
[]
[null,null,null,null,null,null,null,"< Turning gear >"]
[null,null,null,null,null,null,null,"Electric motor :"]
[null,null,"05",{"$f":"D383+1","v":61},null,null,null,"Totally enclosed [IP44]"]
[null,null,"05",{"$f":"D388+1","v":62},null,null,null,"Other / "]
[null,null,"05",{"$f":"D389+1","v":63},null,null,null,"Insulation class [F]"]
[null,null,"05",{"$f":"D390+1","v":64},null,null,null,"Other / "]
[null,null,"05",{"$f":"D391+1","v":65},null,null,null,"Without heater and thermistor"]
[null,null,"05",{"$f":"D392+1","v":66},null,null,null,"With heater"]
[]
[null,null,null,null,null,null,null,"Starter : "]
[null,null,"05",{"$f":"D393+1","v":67},null,null,null,"Supplied by Engine builder",null,null,null,null,null,"(incl. manual remote control box with cable of 15 m)"]
[]
[null,null,null,null,null,null,null,"Receptor for using upper floor :\n"]
[null,null,"05",{"$f":"D396+1","v":68},null,null,null,"Not applied"]
[null,null,"05",{"$f":"D399+1","v":69},null,null,null,"Equipment"]
[]
[]
[null,null,null,null,null,null,null,"< Electric hydraulic oil pump >"]
[null,null,"05",70,null,null,null,"Electric motor : 2sets"]
[]
[null,null,null,null,null,null,null,"Starter :"]
[null,null,"05",71,null,null,null,"Starter is supplied by Shipyard"]
[null,null,"05",72,null,null,null,"Starter is supplied by Engine builder"]
[null,null,null,null,null,null,null,null,"Starting method :"]
[null,null,"05",73,null,null,null,null,null,"Direct on line"]
[null,null,"05",74,null,null,null,null,null,"Other",null,null,"/"]
[]
[]
[null,null,null,null,null,null,null,"< Components, related to LP-EGR* system >"]
[null,null,"05",75,null,null,null,"On-Engine components: supplied by Engine builder"]
[null,null,null,null,null,null,null,null,"Venturi scrubber"]
[null,null,null,null,null,null,null,null,"Demister"]
[null,null,null,null,null,null,null,null,"Scrubbing water reciever"]
[null,null,null,null,null,null,null,null,"EGR blower"]
[null,null,null,null,null,null,null,null,"EGR gas inlet/outlet valve"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"*: Low Pressure - Exhaust Gas Recirculation"]
[]
[]
[null,null,null,null,null,null,null,"< Water treatment system >"]
[null,null,"05",76,null,null,null,"[Water treatment unit], [Collecting tank unit] , [Water cooler unit] and [Control panel] "]
[null,null,null,null,null,null,null,"are supplied by Engine builder"]
[]
[]
[null,null,null,null,null,null,null,"< Other system related to LP-EGR system >"]
[null,null,"05",77,null,null,null,"[NaOH supply system], [Residue discharge system] and [Hull side piping]"]
[null,null,null,null,null,null,null,"are designed and procured by Shipyard"]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,"Engine Seating"]
[null,null,"06","01",null,null,null,"Engine prepared for mounting on epoxy chocks"]
[]
[]
[null,null,null,null,null,null,null,"Epoxy resin chocks :"]
[null,null,"06","02",null,null,null,"Supplied by Shipyard"]
[null,null,"06","03",null,null,null,"Supplied by Engine builder"]
[]
[]
[null,null,null,null,null,null,null,"Holding down bolts/nut :"]
[null,null,"06","04",null,null,null,"Supplied by Shipyard"]
[null,null,"06","05",null,null,null,"Supplied by Engine builder"]
[]
[]
[null,null,null,null,null,null,null,"Foot pieces/caps :"]
[null,null,"06","06",null,null,null,"Supplied by Shipyard"]
[null,null,"06","07",null,null,null,"Supplied by Engine builder"]
[]
[]
[null,null,null,null,null,null,null,"Jack bolt for engine aligment :"]
[null,null,"06","08",null,null,null,"Supplied by Engine builder / Number is engine builder’s standard"]
[null,null,null,null,null,null,null,null,null,null,null,null,null," refer to drawing of [arrangemrnt of holding down bolt]"]
[]
[null,null,null,null,null,null,null,"Trust stopper :"]
[null,null,"06","09",null,null,null,"Supplied by Shipyard"]
[null,null,"06",10,null,null,null,"Supplied by Engine builder"]
[]
[]
[null,null,null,null,null,null,null,"Side stopper :"]
[null,null,"06",11,null,null,null,"Supplied by Shipyard"]
[null,null,"06",12,null,null,null,"Supplied by Engine builder"]
[]
[]
[]
[null,null,null,null,null,null,null,"Lubricating Oil Outlet Position"]
[null,null,"06",13,null,null,null,"Engine bottom :",null,null,null,"Outlet position is Engine builder standard refer to drawing"]
[null,null,"06",14,null,null,null,"Engine bottom :",null,null,null,"Other position  /"]
[null,null,"06",15,null,null,null,"Engine driving end connection "]
[]
[null,null,null,null,null,null,null,"Lubricating oil outlet filter : "]
[null,null,"06",16,null,null,null,"Supplied by Shipyard"]
[null,null,"06",17,null,null,null,"Supplied by Engine builder"]
[]
[null,null,null,null,null,null,null,"Engine Coupling"]
[null,null,null,null,null,null,null,"Engine coupling bolts for thrust shaft and intermediate shaft :"]
[null,null,"06",18,null,null,null,"Supplied by Shipyard"]
[]
[]
[null,null,null,null,null,null,null,"External Conection Flanges "]
[null,null,null,null,null,null,null,"Between engine-side and ship-side :"]
[null,null,"06",19,null,null,null,"JIS"]
[null,null,"06",20,null,null,null,"Other /"]
[]
[]
[]
[null,null,null,null,null,null,null,"Spare Parts"]
[null,null,"07","01",null,null,null,"Spare parts for service required by Engine builder and recommended  \n"]
[null,null,null,null,null,null,null,"or required by the requirements of the classification society \n"]
[]
[null,null,"07","02",null,null,null,"Additional spare parts required by the owner :"]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,"Tools"]
[null,null,"07","03",null,null,null,"Standard tools for maintenance of main engine"]
[]
[null,null,"07","04",null,null,null,"Overhaul tools adapted to: normal lifting procedure, vertical lift of all components"]
[null,null,"07","05",null,null,null,"Overhaul tools adapted to: double jib crane lifting procedure"]
[null,null,"07","06",null,null,null,"Overhaul tools adapted to: reduced height lifting procedure, tilted lift of main components"]
[]
[null,null,"07","07",null,null,null,"Other special tools required by the owner :"]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,"Painting"]
[null,null,"08","01",null,null,null,"Engine builder standard finish : external surface color is [ Munsell 7.5BG7/2 ] "]
[null,null,"08","02",null,null,null,"Other / "]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,"Language"]
[null,null,null,null,null,null,null,"< Name plates for general and caution plates >"]
[null,null,"08","03",null,null,null,"English"]
[null,null,"08","04",null,null,null,"Other / "]
[]
[null,null,null,null,null,null,null,"< Maintenance manual & instruction book >"]
[null,null,"08","05",null,null,null,"English"]
[null,null,"08","06",null,null,null,"Other / "]
[]
[]
[]
[null,null,null,null,null,null,null,"Supervisors Dispatch"]
[null,null,null,null,null,null,null,"During engine installation ~ sea trial / until overhaul inspection :"]
[null,null,"09","01",null,null,null,"Standard :  ",null,null,null,null,null," days / person",null,null,null,null,null,null," number of times"]
[null,null,"09","02",null,null,null,"Other : ",null,null,null,null,null," days / person",null,null,null,null,null,null," number of times"]
[]
[]
[null,null,null,null,null,null,null,"Packing & Transport"]
[null,null,"09","03",null,null,null,"Dispatch pattern : according to consultation result by Engine builder and shipyard "]
[]
[]
[]
[null,null,10,"01",null,null,null,"Other Comment"]
[]
[null,null,10,"02"]